Change Log DentalCAM-Software since Release 3.5.0			
			 
3.5.1		CAM	Finishing of drops in roughening strategy 
			Material PMMA burn added
			
		CNC	CAM 4-K2: tool change optimized
			CAM 4-K:  relieve motion of the spindle adjusted 
			
			
3.5.2		CAM	5 axis drilling strategy added    
			Error in material archive fixed
			
		CNC	CAM 4-K2: tool change optimized
			Drilling of fixing plates for tool changer added   
			5-02: control for the 5 axis module added
			
			
3.5.3		CAM	Error in sinter bar fixed
			Material library depending on OEM 
			
			
3.5.4		CAM	5 axis drilling strategy extended
			
		CNC	signal for indicating error messages
			and operation counter added
			
			
3.5.5		CAM	Transfer protocol between CAM and CNC extended
			Error in the protocol fixed
			
			
3.5.6		CAM	Error in the protocol fixed
			
			 
3.5.7		CNC	Error while importing large objects fixed
			
			
3.5.8		CAM	Prepline extension for safety against raptures
			especially when milling zirconium   
			Warning for objects which are to high adjusted   
			Error in the blank height optimization fixed
			Error in the control of the dust extraction of CAM 4-K2 fixed
			
			
3.5.9		CAM	Height correction of the sinter bar during the blank height optimization
			Error in the preview fixed
			
			
3.5.10		CAM	Height correction of the sinter bar during the blank height optimization
			
			
			
3.5.11		CAM	Slider for rotating objects by mouse/touch screen added
			Error in providing STLs for support folder fixed
			Milling parameters for „PMMA burn“ optimized
			
		CNC	Indication that there is no connection to the machine in the field 
			“machine status”
			
			
3.5.12		CAM	Monitoring, that only one entity can be opened during the calculation   
			in order not to delete the temporary data folder 
			
			
3.5.13		CAM	Special strategy for abutments
			Splitting of the type “Inlay/Abutment” into 2 types
			Optimization of parameters for PMMA
			
		CNC	Protocol window extended if an error occurs during the milling process   
			Error while continuing an interrupted job fixed 
			
			
3.5.14		CAM	Error while finishing the sintering rail fixed   
			Milling parameters standardized 
			
		CNC	Viewer for dongle settings in the menu "Info - Show dongle"
			
			
3.5.15		CAM	Milling parameters for fully anatomical objects optimized
			English translation completed
			
		CNC	Error in country settings fixed
			Protocol will no longer be overwritten when updating
			(operation counter, milling protocol)
			English translation completed
			
			
3.5.16		CAM	Protocol CAM/CNC access conflict fixed
			Collision control while finishing bars for 
			deep-seated bars in high blanks inserted
			4/5 axis strategies activated
			Parameters for Model base and Model inserting tooth added
			
			
		CNC	Error in marking blank position fixed
			
			
3.5.17		CNC	Error in relieve motion after moving the A axis with an external CAM f
			ixed
			
			Reminder for change-over at CAM 5-02 extended
			
			
3.5.18		CAM	Error in calculation of the milling path fixed
			Error in automatically equipping the tool changing unit fixed
			
			
3.5.19		CAM	Error in calculation of the milling path (finishing, error 6) fixed
			
			
3.5.20		CAM	Calculation of drilling centres for 5 axis drilling optimized
			
		CNC	Maximum endurance in the operation counter editable.
			
			
3.5.21		CNC	Change of the axis slant for CAM 5-02
			
			
3.5.22		CNC	Saving of data into the controller minimized
			Individual tool names and endurances
			
			
3.5.23		CNC	Error in „Continue job“ fixed
			Editing of tool endurances only in administrator mode possible
			
			
3.5.24		CAM	OEM material adaption
			
		CNC	Number of ignored measuring points in the calibration set to 2.
			
			
3.5.26		CNC	Error while transferring ini file using Windows 7 fixed
			
			
3.6.0		CNC	Error while measuring/plane-milling the measuring key fixed
			Error in tool breakage monitoring fixed
			Error while continuing an job with CAM 4-K1 fixed
			
			
3.6.1		CNC	Error while manually changing tools with CAM 4-02 fixed
			
			
3.6.2		CNC	Window size adjusted for the resolution 1024x600
			
			
3.6.3		CAM	Both-sided usage of the 0.6 mm cutter for inlays, in each quality
			OEM adaptions
			
			
3.6.4		CAM	Search for drillings for abutments optimized
			
		CNC	Dongle information only shown in administrator mode
			Breakage monitoring changed
			
			
3.6.6		CAM	Error after updating fixed
			
			
3.6.7		CNC	Error in position of the A axis of CAM 4-K1 fixed
			
			
3.6.8		CNC	OEM adaptions
			
			
3.6.9		CAM	Error in calculation of the drillings of abutments fixed
			
			
3.6.10		CNC	Measuring of tool changer, Z value optional
			Manual tool change modified
			Cleaning instruction previous to the calibration
			
			
3.6.11		CNC	Breakage monitoring changed
			
			
3.6.12		CNC	Manual tool change – error fixed
			
			
3.6.13		CAM	Scaling zirconium – error fixed
			
			
3.6.14		CNC	Error in measuring of tool changer fixed
			
			
3.6.15		CNC	Error while measuring the tool changer of CAM 5-02 fixed
			
			
3.6.16		CAM	Bars of deleted objects are blanked out
			Import of 3Shape files
			
		CNC	Cleaning of the working area of CAM 4-K2 – macro inserted
			
			
3.6.17		CAM	Bar code scanner added
			Milling parameters modified
			
			
4.0.0		CAM	Auxiliary line for positioning for 4 axis finishing extended for CAM 4-00
			
		CNC	Compressed air and traffic light display, if compressed air is lacking
			Support folder is deleted on the start of a job, to prevent having out-
			dated data
			
			
			
4.0.1		CAM	OEM adaptions
			Setting bars – error fixed
			
		CNC	Deleting support folder – error fixed
			
			
4.0.2		CAM	Error in data base (lot number) fixed
			
			
4.0.3		CAM	OEM adaptions
			
		CNC	Printout of the machine geometry in a text file (...\MG.txt)
			
			
4.0.4		CNC	Modification tool breakage monitoring
			
			
4.0.6		CAM	OEM adaptions
			
			
4.0.8		CAM	OEM adaptions
			
		CNC	OEM adaptions
			
			
4.0.9		CAM	Sorting feature for STLs in the import window by clicking onto the 
			column heads (name, size, date)
			
		CNC	OEM adaptions
			
			
4.0.10		CAM	OEM adaptions
			
		CNC	Adaptions for UL machines
			
			
4.0.11		CAM	Preview adjusted (mirror-inverted)
			
			
4.0.12		CAM	Preview on request only (button)
			OEM adaptions
			
			
4.0.13		CNC	Adaptions for UL machines (dust extraction)
			Postion for measuring the measuring key moved for machines of the K 
			series
			OEM adaptions
			
			
4.0.14		CNC	Cleaning reminder previous to start of milling process – deselectable 
			in settings
			
			
4.0.15		CAM	OEM adaptions
			
			
4.0.16		CAM	Calculation of drillings of abutments modified
			
			
4.0.17		CAM	OEM adaptions
			
			
4.0.18		CAM	OEM adaptions
			
			
4.0.19		CNC	Switching output enabled for CAM 4-K4

4.0.20		CNC	OEM adaptions
